# `colorsys` --- 色体系間の変換

ソースコード: Lib/colorsys.py

The `colorsys` module defines bidirectional conversions of color values between colors expressed in the RGB (Red Green Blue) color space used in computer monitors and three other coordinate systems: YIQ, HLS (Hue Lightness Saturation) and HSV (Hue Saturation Value). Coordinates in all of these color spaces are floating-point values. In the YIQ space, the Y coordinate is between 0 and 1, but the I and Q coordinates can be positive or negative. In all other spaces, the coordinates are all between 0 and 1.

参考

色空間に関するより詳細な情報は https://poynton.ca/ColorFAQ.html と https://www.cambridgeincolour.com/tutorials/color-spaces.htm にあります。

`colorsys` モジュールでは、以下の関数が定義されています:

colorsys.rgb_to_yiq(r, g, b)

  RGB から YIQ に変換します。

colorsys.yiq_to_rgb(y, i, q)

  YIQ から RGB に変換します。

colorsys.rgb_to_hls(r, g, b)

  RGB から HLS に変換します。

colorsys.hls_to_rgb(h, l, s)

  HLS から RGB に変換します。

colorsys.rgb_to_hsv(r, g, b)

  RGB から HSV に変換します。

colorsys.hsv_to_rgb(h, s, v)

  HSV から RGB に変換します。

以下はプログラム例です:

    >>> import colorsys
    >>> colorsys.rgb_to_hsv(0.2, 0.4, 0.4)
    (0.5, 0.5, 0.4)
    >>> colorsys.hsv_to_rgb(0.5, 0.5, 0.4)
    (0.2, 0.4, 0.4)